BusinessPhone Communication Platform 5.1
Commands > Commands 4000...4999

## 4005
Auto. answer superv. time

This command is used to state the supervision (monitoring) time for calls to the operator in conjunction with automatic answer. If the operator does not press any function key within the stipulated time, the call will be cleared down and the operator will be marked “off duty”.

Range of values = 0-11 min

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003