BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1919
Assigned TEI value

The command is used to assign a TEI, Terminal Endpoint Identifier value for the Basic Rate Access ISDN-link (Q-/T-interface). This command is used if a non-automatic assignment shall be used, i. e. a programmed TEI value. If automatic assignment exists, which means that TEI value will be received from the network on request, no programming shall be done. The ‘undefined’ TEI value will inform the trunk to make request to the network.

Value:

FFh = undefined, not valid assigned/not programmed

TEI value 00-63 = valid assigned TEI values

Used initial value

(T): FFh = undefined, see above

(Q): 00

This command is only programmable for T-interface!

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003