BusinessPhone Communication Platform 5.1
Commands > Commands 9000...9999

## 9147
IP address reference 4

This command is used if the route choice is based on a VoIP connection. The reference number refers to a command table entry comprising the IP number of the destination node (see command 2163 Signaling protocol, 2164 Network IP address).

##### Valid data

0 (default) |  | not programmed |
1-1000 |  | valid IP reference number |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003