BusinessPhone Communication Platform 5.1
Commands > Commands 8000...8999

## 8203
Receiver type

This command is used to determine the type of paging receiver.

0 = “Bleeper” type receiver without display |  |

1 = Display receiver for call-me paging |  |

2 = Receiver with speech option without display |  |

3 = Receiver with speech option with display |  |

4 = Group call without display |  |

5 = Group call with display |  |

6 = Display receiver for meet-me paging |  |

For standard paging the receiver type is used to determine the type of paging to be started.

For alternative paging, a check takes place to verify that the requested paging can be handled by the receiver.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003