BusinessPhone Communication Platform 5.1
Commands > Commands 3000...3999

## 3102
Name for Loudspeaker paging group 0

The command states which name text is to be shown on display telephones in the PABX with calls to a loudspeaker paging group.

Valid values: 20 characters (ACSII)

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD4 © Ericsson Enterprise 2003