BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0x5D
No TR-Buffer

Default definition: |  | ERROR |
Used by block: |  | TR |
Category: |  | DESIGNER |

The buffer already exists, no buffer has been available or it was not allowed to keep the buffer.

- D1: Process or device state
- D2: Message code
- D3: Undefined
- D4: Undefined

Revision: PH2 © Ericsson Enterprise 2003