BusinessPhone Communication Platform 5.1
Dialogs

## Trunks

The “Trunks” menu comprises functionality for all kind of trunks in a connected or loaded system. BMS knows the following trunk types:

- Analog
- CAS
- ISDN
- IP

Each trunk type is represented by a submenu to provide a better overview for selection and navigation.

The following options are available via the trunk context menu:

- List Trunks - System Trunk Assignment

- Depending on the selected trunk type, all existing trunks in the system of the selected type are displayed.

- Assign Trunks

- This dialog gives an overview about the system trunks and is also used to assign trunks.

The following operation can be applied only for ISDN trunks:

- ISDN Interface Type Assignment

- You can assign an interface type for the ISDN links of the system. Possible interfaces are T, Q and S interfaces.

Note

When one of these operations is applied on the superior trunk menu, all trunks in the connected or loaded system are included in the selected operation.

Furthermore, the “Trunks” menu offers access to:

- X.25 - Packet Mode Communication (packet mode communication)
- Trunk Routes

Revision: B © Ericsson Enterprise 2003