BusinessPhone Communication Platform 5.1
Facilities

## Bypass Call Diversion and Follow Me

## Definition

If an extension has activated call diversion or follow me, you can bypass call forwarding by dialling a specific code.

## Use

Bypass call diversion and follow me makes it possible to call a specific extension, even if call forwarding is activated on this extension.

Calls to internal directory numbers via the public network or private network have the possibility to be translated into DDI numbers by the individual number translation table.

For further information please refer to the document Individual Number Translation on page 1 (170/155 34-ASB 150 02 Uen).

## Operation

If there is any kind of call forwarding (=diversion direct, diversion on busy, diversion on no reply or follow me) active on an extension, calls to this extension will automatically be routed to the programmed directory number.

Note

For more information concerning "call forwarding" see "diversion direct", "diversion on busy", "diversion on no reply" or "follow me".

If you have the permission, active call forwarding to another directory number can be bypassed. In that case the dialled extension will be called, no matter whether it has activated diversion direct, diversion on busy, diversion on no reply or follow me.

If you want to call an extension without being forwarded to another directory number, the following procedure has to be applied:

- Lift the handset. (Not necessary for EXECUTIVE, STANDARD and ECONOMYplus Telephones)
- Dial *60*xxxx# (xxxx = extension number)

- You will be connected to the specified extension, no matter if it has activated diversion direct, diversion on busy, diversion on no reply or follow me.

## Capacity

All extensions, which have activated call forwarding, can be called directly without being diverted.

All guest extensions, which have activated "Do not disturb" can be called.

## Limitations

Bypass call diversion and follow me can only be used from extensions. It can not be used from the operator and from fictive numbers.

The operator has for this purpose his own Bypass-key.

## Programming

3082 |  | Bypass call diversion

## Equipment

No additional hardware necessary.

Revision: G © Ericsson Enterprise 2003