BusinessPhone Communication Platform 5.1
Dialogs

## Edit Carrier

In this dialog you can configure all carrier specific settings. To access the dialog, open the “Facilities” menu in the Configuration directory tree. Then open the “Least Cost Routing” submenu and click on “Carrier”. The Carrier dialog opens. Now click on a carrier’s link, for example on “Carrier 1”.

The dialog consists of four sections:

- General
- Detecting area access code
- Destination number modification
- Arranging number to send

If you need more information about a setting or a field, click on the command link in brackets.

### General table

The General table defines all access related settings of a carrier:

8436 |  | Carrier name

8401 |  | Internal access code

8402 |  | Predigits for carrier access

8403 |  | Billing principle

### Detecting carrier access code table

You can define up to 16 different carrier access codes. For each carrier, a public number can be entered as well.

8405 |  | Detecting carrier access codes

### Destination number modification

This table is used to retrieve the B-number that is sent to the carrier network. Up to 16 different settings can be configured. Besides, the table defines the corresponding external access code for a carrier.

##### Example:

A carrier offers only international destinations, starting with 00. The external access code for the carrier network is 190. To prevent the system from dialing unnecessary digits the carrier has further specified that the two leading digits (00) must not be dialed. In this case, the carrier configuration would look like this:

- Destination number: 00
- Delete: 2
- Carrier Access Code: 190

### Arranging number to send

Using the drop-down list boxes you can define the form of the number that is sent to the carrier network. Up to 8 number components can be specified:

- B-number
- External access code
- Authority code
- Account code
- Own extension number
- Change to DTMF
- Wait for Proceed To Send tone
- Delay time

The parameter setting on the right is only available for the delay time selection.

#### Actions

Submit |  | To send the settings to the system. |
Reload |  | To load the current system settings and to discard all entered data or changes. |
Delete |  | To delete the currently selected carrier. |
Carrier List |  | To return to the Carrier dialog. |

Revision: B © Ericsson Enterprise 2003