BusinessPhone Communication Platform 5.1
Commands > Commands 3000...3999

## 3304
First alternative route

When all trunks between two exchanges are busy, the call can be sent via another exchange. An alternative route shall be defined for the call to be rerouted. Two different alternative routes can be defined. The first alternative route is defined with command 3304. The second alternative route is defined with command 3306 Second alternative route.

Valid Values: Trunk route directory number

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD4 © Ericsson Enterprise 2003