BusinessPhone Communication Platform 5.1
Commands > Commands 5000...5999

## 5409
Create fictive directory number series

It is possible to define “fictive directory numbers” in ASB 150. The fictive directory number facility means that all calls to the number are queued. If there is a call queue, this is indicated on all telephones that have a programmable key for monitoring the fictive number.

With this command a fictive directory number with a stated number can be created.

The facility can be assigned to any free directory number not conflicting with existing directory numbers.

ASB 150 permits a maximum of 16 fictive directory numbers.

Valid values: 4 digits (0-9,*,#,-)

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: C © Ericsson Enterprise 2003