BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0x34
Invalid Signal Number In Message

Default definition: |  | ERROR + TRIG |
Used by block: |  | ALL |
Category: |  | DESIGNER |

The signal number (SN) in the message was not valid.

- D1: Received signal number (SN)
- D2: Received INFCODE
- D3: Received SUBCODE
- D4: Received DATA+1

If ‘OS.WARNING code,DY’ is not used, data D3 and D4 are supplied by OS from the ME-register.

Revision: PH2 © Ericsson Enterprise 2003