BusinessPhone Communication Platform 5.1
Commands > Commands 6000...6999

## 6205
Bar outgoing calls for guest

The command is used for prohibit or allow outgoing calls for guest extensions, if the memory for call records reaches its full capacity.

When external equipment is switched off, all the call and hotel records which will be sent to the v.24 port will be stored. If CPU-D3 or higher is used, the records will be stored in a non volatile memory and the records also will remain in the memory after a system restart.

The command is valid for CPU-D3 and higher versions.

##### Valid data

Yes |  | If memory is full, prohibit outgoing calls for guest extension |
No |  | If memory is full, outgoing calls are allowed for guest extension |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2003