BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0x9C
Heartbeat Failed

Default definition: |  | ALARM |
Used by block: |  | OM |
Category: |  | MAINTENANCE |

The code is used, when the heartbeat function failed.

- D1: Type of error

- 10h: Timer request failed, no heartbeat sent.
- 11h: Unable to seize port, no heartbeat sent
- 12h: No connection, no heartbeat sent
- 13h: No answer to heartbeat

- D2: 0
- D3: Undefined
- D4: Undefined

Revision: I © Ericsson Enterprise 2004