BusinessPhone Communication Platform 6.0
Commands > Commands 3000...3999

## 3079
Malicious call id

This command specifies which A-category/categories is/are allowed to request malicious call identification, i.e. to request the network to store details of the originator of the call.

Malicious call identification is an ISDN facility. The request can be made during the active state or during the disconnect state of the call. It is only the terminating party that can make the request.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004