BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0x9A
Backup Battery Used

Default definition: |  | INFO + NOPROG + EXTERN + ACTIVE |
Used by block: |  | OM |
Category: |  | MAINTENANCE |

The code is used, when a signal on the alarm input on the CPU card is detected. This input is used to notify the system, that the backup battery is currently being used.

- D1:
- D2:
- D3: Undefined
- D4: Undefined

Revision: I © Ericsson Enterprise 2004