BusinessPhone Communication Platform 6.0
Dialogs

## X.25 - Packet Mode Communication

You can configure the packet mode communication links used for X.25 for up to 3 boards equipped with ISDN BA.

To select the configuration dialog of a board, open the “Trunks” menu in the Configuration directory tree and click on the “X.25” submenu to open the context menu.

The configuration dialog consists of a list of system cards that may be configured for PMC links. Depending on the system card (BTUB 8/16 or MFU), the number of programmable PMC links and the number of potential ISDN BA interfaces is restricted.

You can group the ISDN interface links of a card for X.25 packet transfer. An interface link consists of the ISDN BA interface number on the card and a used TEI value.

Note

An interface link can only be used once for one card.

To delete the PMC configuration of a board, just click on the Submit button below without selecting a card.

For more information, please see command:

1980 |  | Packet Mode Communication Link parameters

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To reload the current system parameters. |

Revision: F © Ericsson Enterprise 2004