BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1710
Seizure acknowledge

The command is used to state whether the line signal “seizure acknowledge” shall be received (exists) at an outgoing call.

Note

Ascertain that the signal is included in the selected line signal scheme.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004