BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0x13
Invalid Signal Type In Message

Default definition: |  | ERROR + TRIG |
Used by block: |  | OS |
Category: |  | DESIGNER |

The signal type (ST) in the message was not valid.

- D1: Job identity of the sender (usually signal type ST)
- D2: Received INFCODE
- D3: Received SUBCODE
- D4: Received DATA+1

Revision: I © Ericsson Enterprise 2004