BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1311
Number of digits before EOS-signal

The command is used to determine the number of received digits for automatic incoming traffic before sending the EOS-signal to the superior exchange, e.g. a predetermined number of digits is always received before the EOS-signal is sent. Value 1-4 digits.

If no value is stated, the EOS-signal will be sent as soon as the ordinary number analysis states that a complete number has been received irrespective of the number of digits.

##### Valid data

1 |  | (default) |
2-4 |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004