BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2178
GK NGK heart beat time interval

Length of the time interval between two heart beat actions invoked towards a neighbourhood gatekeeper for the health check purpose.

##### Valid data

1-255 |  | minutes |
10 |  | default |

Note

There is no possiblity to deactivate the heart beat feature to increase performance

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004