BusinessPhone Communication Platform 6.0
Commands > Commands 7000...7999

## 7431
Active alarm I/O port

The command determines the I/O port to be used for the sending of active alarms.

The I/O-port should be entered as: ppiii

where

pp = Position of circuit board (00-63) |  |

iii = Individual number |  |

of a V24 (IO Unit) port. |  |

‘Active alarm’ is a function which transfers alarms to an external alarm receiver.

Commands 7420 Service area id, 7421 Identity of exchange and 7430 Active alarm on?-7437 Max active alarms per day concern active alarms.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2004