BusinessPhone Communication Platform 6.0
Commands > Commands 5000...5999

## 5510
Delete call number for standard paging

ASB 150 permits connection of external equipment for paging via radio or a magnetic loop. Connection takes place via a trunk (external line) board that has been reserved for this purpose.

This command is used to delete the call number for standard paging.

Standard paging means that paging takes place with the “meet-me” or “call-me” principle without the pager being able to transmit his/her own orders to the paging receiver.

Commands 5511 Delete call number for alternative paging and 5512 Delete answer number for meet-me are used to delete other directory numbers (if any) that have been created for paging.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004