BusinessPhone Communication Platform 6.0
Dialogs

## Assign Master/Slave

You can assign a primary and secondary telephone for a Tandem configuration. All types of extensions - analogue, digital, and cordless extensions - can be part of a Tandem setup. The dialog shows all system extensions that are available for a Tandem configuration.

To access the dialog, click on the “Extensions” menu in the Configuration directory tree to open the context menu. Then select “Assign Master/Slave” to open the Master/Slave Extension Assignment dialog. Alternatively, select the “Assign Master/Slave” option in one of the “Extensions” submenus (e.g. Analog, Cordless, or Digital).

For more information about this feature, see also:

facility description Tandem Configuration (480/15534-ASB 150 02 Uen).

5630 |  | Assign master/slave.

### To assign a slave telephone

- To assign a secondary telephone, enter the relevant extension number in the “Slave” field.
- Click on Submit.

### Changing the extension’s parameters

- Select a directory number with the Directory Number drop-down list box.

- Or

- Enter the extension number directly in the field beneath the drop-down list box.
- The Extension Parameter opens. Here you can set up the extension’s details. For more information about this dialog, please see section Extension Parameter.

#### Actions

Submit |  | To transmit the settings to the system. |
Reload |  | To reload the current parameters. |

Revision: B © Ericsson Enterprise 2004