BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2171
Gatekeeper activated?

This command defines whether or not the Gatekeeper function is actived on the selected IPU board. If modified, a restart of the IPU is required.

If modified, a restart of the IPU is required.

##### Valid data

Yes |  | The Gatekeeper is activated |
No (default) |  | The Gatekeeper is not activated |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004