BusinessPhone Communication Platform 6.0
Commands > Commands 6000...6999

## 6502
Listing of data for directory numbers

A printout of the programmed dataposts is done. The assignment of a namestring to a non guest directory number is done with the command 6501 Directory name.

A datapost for guests is prepared by doing a check in (by hotel function key * 31 #).

Command 6011 Autoselect allowed of the connected printer must be set to YES.

Three types of printout can be ordered:result.

Value |
ALL | Dataposts for guest and non guest extensions are printed.
GUEST | Dataposts for guest extensions are printed.
DIR | Dataposts for all non guest extensions are printed.

Minimum required authority level from telephone: 1

Accessible via BMS: No

Revision: E © Ericsson Enterprise 2004