BusinessPhone Communication Platform 6.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## C9 CILCONREL

0 RER.NOTS |  | Not specified |
1 RER.TFR |  | Transfer |
2 RER.DNR |  | Diversion on no reply |
3 RER.BRK |  | Break in |
4 RER.CNF |  | Conference |
5 RER.OPR |  | Operator recall, after 'parked by operator' |
6 RER.NIN |  | Information not available |
7 RER.MG |  | Reroute call to MG |
8 RER.TFRBFA |  | Transfer before answer |
9 RER.CB |  | Call back |
10 RER.ACD |  | Reroute of ACD-call |
11 RER.SIL |  | Reroute on silent intrusion |
12 RER.BRKKEEP |  | Reroute, break in, keep display |
13 RER.LCRRDY |  | Least cost routing ready |
14 RER.LCRREQ |  | Least cost routing request |
15 RER.COBEXT |  | Reroute common bell extension |
16 RER.CANSWPOS |  | Exit storing and retrieving of messages |
17 RER.NMSG |  | Override multiple diversion to MG |
18 RER.FACEXIT |  | Exit from a facility to the desired directory number |
19 RER.CTI |  | Reroute caused by CTI |
20 RER.BYP |  | Reroute bypassing call diversion |
21 RER.DNA |  | Diversion on cordless not available |
22 RER.CNBYP |  | Reroute bypassing call diversion at calls to a CN party |
23 RER.CNDNR |  | Reroute on no reply to a CN diverted-to party |
24 RER.CNDIV |  | Reroute on CN call diversion immediate, on busy or on no reply when diverting party is another PBX |
25 RER.FACBUSY |  | Reroute from facility to exit position because the desired party is busy |
26 RER.CNDNA |  | Diversion on cordless not available to a CN diverted-to party |
27 RER.CONREC |  | Reroute on conversation recording |
28 RER.3PTYCONF |  | Reroute request to EX/OP from TR |
29 RER.OCN |  | Reroute on outcall notification |
30h CLREGNEW |  | Release, start with new regtone |
31h CLREGKEEP |  | Release, start with new regtone, keep proc |
32h CLCBBOOK |  | Release, book for specified party |
60h CLSZBOOK |  | Call rerouted or transferred |
61h CLMETER |  | Update metering information |
62h CLCONSENT |  | CONREL is sent and connection released |
63h CLCONREC |  | CONREL is received and connection released |
90h CLBUFCONG |  | Free logging buffer not available |
91h CLACCONG |  | Account code not dialled |
92h CLACCERR |  | Faulty account code dialled |
93h CLCFPR |  | Partial rerouting |

Revision: F © Ericsson Enterprise 2004