BusinessPhone Communication Platform 6.0
Commands > Commands 4000...4999

## 4104
Receiving of tone signals

The command defines if the operator should receive tone signals during traffic indicating several cases in addition to the indication on the display.

Alternatives:

NO: Additional tone signals are disabled. The operator will receive the display information for several traffic cases. |  |

YES: The operator will receive tone signals. |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004