BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1023
Trunk line type

The command is used to state to which type of trunk the BTU is connected.

##### Valid data

0 |  | Trunk to a public exchange (PE) |
1 |  | Trunk from a public exchange with direct in-dialing (INDIALING) |
2 |  | Trunk to a private exchange, tie line (TIE LINE) |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004