BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2107
Wait for answer for data calls

In case of a data call from one extension to another, the call will be disconnected after a certain period of time, if the extension does not answer.

This command determines the time after which the call shall be disconnected.

0 = No time monitoring |  |

1-255 = Answer time in seconds. |  |

Minimum required authority level from telephone:

Accessible via BMS:

Revision: G © Ericsson Enterprise 2004