BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2094
GAP Version

This command defines which version of GAP protocol should be used for communication with cordless phones.

For software releases R10, R11 GAP 1.x has to be programmed,(GAP 2.0 not supported) software releases R12 and higher support GAP 1.x and GAP 2.0 protocol.

NOTE: If the parameter is changed while the system is in operation, the IC-CU2 has to be reinitiated or a system restart has to be performed.

##### Valid data

1 = GAP 1.x, 2 = GAP 2.0

Default data: 2 = GAP 2.0

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004