BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0x64
Invalid Parameter(s) To BTU

Default definition: |  | ERROR + TRIG |
Used by block: |  | TR |
Category: |  | MAINTENANCE |

The BTU did not accept the E2 data, sent to it. If this happens during a coldstart, the BTU will use its own default parameters. If it happens during programming, no change are made to the current parameters. The second parameter contains information about the not accepted data at the parameter updating to the RP. The RP replies with the internal number value for the parameter.

- D1: SUBCODE for the actual parameter updating code.
- D2: Internal parameter number value for not accepted data.

- 01h: Signal interface scheme, scheme is not available on the RP
- 02h: Dial tone level, level out of range
- 03h: Disconnection tone level, level out of range
- 04h: Filter coefficient, filter coefficient not available
- 05h: Relative send level, level out of range
- 06h: Relative receive level, level out of range
- 07h: Network / User, level out of range
- 08h: Already assigned packet mode link
- 09h: Already assigned TEI for an interface

- D3: Card position
- D4: Individual number of BTU

#### Recommended action

Check revision/version of the RP (and/or BTU).

Revision: I © Ericsson Enterprise 2004