BusinessPhone Communication Platform 6.0
Commands > Commands 4000...4999

## 4008
Calling of extension at incoming call

This command gives an opportunity to determine what will happen in the following traffic case:

There is an answered incoming call on the left side and the operator has called a free extension on the right side. The operator has not initiated ringing yet. At this moment the extension (on the right side) lifts the handset or answers in any other way.

Alternatives:

0 = There will be a three-party connection between the operator and the left and right side parties. |  |

1 = The extension will be parked by the operator. |  |

2-9 Reserved |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004