BusinessPhone Communication Platform 6.0
Facilities

## Register Recall In PSTN

## Definition/Use

Inquiry, Refer back and Conference can be established on a system telephone without using a second external line.

## Operation

By pressing the programmable R-key on a system telephone, the following features are available:

- Inquiry on the same external line
- Refer back
- Conference

These features can be used on the same line, which is a great advantage as compared to the PBX functions, where always two external lines will be occupied for achieving the same functionality.

During suffix dialling, a TCD check that differs from the normal TCD check is performed.

## Capacity/Limitations

The register recall can be done from all system telephones with programmable keys.

DBC 220 |  | 4 |
DBC 222 |  | 4 |
DBC 223 |  | 4 |
DBC 224 |  | 3 |
Old telephones
DBC 210 |  | 3 |
DBC 211 |  | 4 |
DBC 212 |  | 4 |
DBC 631 |  | 10 |
DBC 213 |  | 14 |
DBC 662 |  | 30 |
DBC 214 |  | 3 |
DBC 663 |  | 20 |

The access to functions in the public net is always dependent on functionality provided by the network provider. This document only refers to functions which will be activated via analogue trunks

## Programming

0301 |  | Function of programmable key

Enter the function code = 25

0179 |  | TCD suffix dialling-day COS

0180 |  | TCD suffix dialling-night COS

These commands are only accessible via BMS:

1417 |  | Length of external inquiry signal

2088 |  | TCD for suffix dialling when authority code active (day-switched)

2089 |  | TCD for suffix dialling when authority code active (night-switched)

## Equipment

System Telephone.

Revision: D © Ericsson Enterprise 2004