BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0x9B
Card Missing After Powerup

Default definition: |  | STOP |
Used by block: |  | OM |
Category: |  | MAINTENANCE |

The code is used, when the supervision function found a missing card after power-up. Missing is defined as present in the E2 area, but does not report at start-up. This warning is sent only at the power-up restart.

- D1:
- D2: Card position for the first missing card
- D3: Undefined
- D4: Undefined

Revision: I © Ericsson Enterprise 2004