BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2164
Network IP address

Defines the IP address of the nodes (up to 1000) within the network, and includes also the corresponding port number for the defined application. The "1000 node" table is used for configuration of gateways which are operated without consulting the gatekeeper.

##### Valid data

Network IP adress |  | Port |
0.0.0.0 - 255.255.255.255:(0 - 65535) |  |  |
0.0.0.0:0 ( default) |  |  |

Note

The predefined call signalling Port number (Q.931) for ASB 150 02 IP Gateways is 7000 (see command 2162 Port number in the destination node). If you change the port number to another value, please take in considuration that this port number always has to correspond to the port number defined in the destination node.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004