BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0xCC
CN Alternative Route Used

Default definition: |  | UNDEFINED |
Used by block: |  | TR |
Category: |  | MAINTENANCE |

An outgoing CN call was cleared by the network because of a special network related reason and a new call setup attempt over the next PNR route choice is done.

- D1: Card position
- D2: Individual number
- D3: Directory number of PNR, high byte
- D4: Directory number of PNR, low byte

Revision: I © Ericsson Enterprise 2004