BusinessPhone Communication Platform 6.0
Commands > Commands 8000...8999

## 8702
Error-announcement reference

In this command you must specify the identification number of the “Error announcement”.

Press Enter to go to the next command of the current selections list.

Note

Do not forget to record voice announcements first (see command 4411 Command to record the new AA announcement group).

##### Valid data

1-42 |  |  |
(blank) |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2004