BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0164
DID to extension enabled?

The command defines whether or not an extension should be allowed to receive an external call (DID) directly. If set to ‘no’, DID calls will be rerouted. For hotel guest room extensions, the call is rerouted to the hotel answering position. Calls to all other extensions are rerouted to the trunk answering position. The answering position is allowed to transfer DID calls to extensions even if they are blocked for DID calls.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004