BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0158
Diversion on busy at external calls ?

The command defines whether or not a diversion on busy on an external incoming call should be done.

If the extension is a master and a member of a tandem configuration the command data shall be copied to the slave and blocked for the slave's futher use.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004