BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2610
Number of DTMF tones

This command determines the number of DTMFs to be 12 or 16. If the number of DTMFs is 16, the maximum number of tone fragments is 15. If the number of DTMFs is 12, 19 tone fragments are possible (see command 2601 Tone fragment definition).

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004