BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0xC8
CM Meter Limit Exceeded

Default definition: |  | ALARM + INFO |
Used by block: |  | CM |
Category: |  | MAINTENANCE |

The call meter function accumulates the total cost and number of received tax pulses for both, the originator and the trunk of all outgoing external calls. The directory numbers of the originator and the trunk are used as identifiers of the accumulators. This warning indicates, that the limit, specified with command 6713 (Cost Limit), has been exceeded for a certain cost accumulator.

- D1: Directory number of the accumulator, high byte
- D2: Directory number, of the accumulator, low byte
- D3: Undefined
- D4: Undefined

#### Recommended action

Read and reset the call meter for the appointed directory number.

Revision: I © Ericsson Enterprise 2004