BusinessPhone Communication Platform 6.0
Commands > Commands 6000...6999

## 6901
Common bell extension

Here you can define the extension which is used as common bell extension.

Insert the call number (directory number) of the selected extension.

The common bell extension is the telephone from where all other extensions will pick up the call by dialling the common bell pick-up code. Only one common bell extension can be created for the whole system.

The operator cannot be a common bell extension because it is not allowed to pick up a call to an operator extension.

Further picking-up is not possible if connection is prohibited by the traffic group.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004