BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0115
Ringing line 2

The command states which form of ringing shall present incoming calls on LINE 2.

0 = No ringing

1 = Ringing

2 = Ringing after 10s delay

3 = Only first ringing period, suppressed

4 = Only first ringing period, suppressed after 10s delay

If the extension is busy when the ringing signal is to be sent, only one ringing period is sent, suppressed even if the line is programmed for ringing.

Ringing can also be altered by extension users themselves via individual programming.

##### Valid data

0-1 |  | (default) |
2-4 |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004