BusinessPhone Communication Platform 6.0
System Overview ASB 150 02 Release 14 (BusinessPhone 6.0)

## Technical Data

- Mechanical Characteristics
- Electrical characteristics
- Capacities
- Telephones
- Door interface unit
- Trunks
- Tie lines
- Transmission data
- CTI
- Networking
- DECT Radio Interface
- Compliance Information

### Mechanical Characteristics

Note

All dimensions given in length x width x height.

| dimensions | weight
#### Cabinets
BDVBS 101 05 (BP50) | 500 x 400 x 155 mm | 13,00 kg
BDVBS 101 06 (BP128i) | 482,5 x 396 x 124,5 mm | 14,50 kg
BDV 113 08 (BP250) | 260 x 435 x 300 mm | 19,20 kg
#### Telephones
DBC 220 | 230x 159 x 102 *) mm | 0,63 kg
DBC 222 | 230 x 159 x 102 *) mm | 0,67 kg
DBC 223 | 233 x 204 x 102 *) mm | 0,84 kg
DBC 224 | 234 x 240 x 102 *) mm | 1,0 kg
DBC 425 | 234 x 240 x 102 *) mm | 1,0 kg
DBY 419 02 (key panel) | 226 x 64x 90 *) mm | 0,22 kg
DBC 106 | 230x 159 x 102 *) mm | 0,78 kg
DBC 147 | 230 x 159 x 102 *) mm | 0,78 kg
#### Auxiliary equipment
DIU | 100 x 170 x 40 mm | 0,25 kg
Desktop Adapter | 152 x 33 x 75 mm | 0,15 kg

*) telephone set with feet in lowest position

### Electrical characteristics

#### Radio interference

CE regulation: |  | 89/336/EEC |
complies to EN 55022, Class B

#### Power supply BP50/ BP128i

Mains voltage: |  | 110-127 VAC ±10% |
Input current max.: |  | 3A (4A with battery charger) |
Mains voltage: |  | 220-250 VAC ±10% |
Input current max.: |  | 1.5A (2A with battery charger only BP50) |
Safety: complies to safety class I acc. to EN 60950, LVD 73/23/EEC

#### Power supply BP250

Switched mode power supply

Mains voltage: |  | 110-127 VAC ±10% |
Input current max.: |  | 6A |
Mains voltage: |  | 220-240 VAC ±10% |
Input current max.: |  | 3A |
Safety: complies to safety class I acc. to EN 60950, LVD 73/23/EEC

##### Transformer

Mains voltage: |  | 110-127 VAC ±10% |
Input current max.: |  | 6A |
Mains voltage: |  | 220-240 VAC ±10% |
Input current max.: |  | 3A |
Safety: complies to safety class I acc. to EN 60950, LVD 73/23/EEC.

#### Alternative power feeding for BP250

|  | 36 VAC ±4 V 50 Hz 48 VDC +8 V/-5 V |

#### Environmental requirements

Ambient temperature |  | 5 - 40˚C |
Humidity |  | 15 - 80% |
Electrostatic discharge |  | 15 kV at 30% humidity |
complies to IEC801-2 |  |  |

#### Data communication interfaces

V.24 (RS-232C) |  | up to 19,2 Kbit/s |
Range |  | up to 15m |
RS-485 |  | up to 1200 m. |

### Capacities

#### Switch capacity

ASB 150 02 supports a maximum of speech 60 channels.

Speech channels can either be used on request for the normal traffic between an originator and a terminator or they can be permanently assigned to features such as Music on Hold and Background music.

In case of the normal traffic a maximum of 120 individuals can be involved in a:

- Trunk to Trunk connection (Route)
- Trunk to Tieline connection (Network-Node)
- Trunk to S-Terminal connection
- Trunk to Voice over IP gateway connection
- Trunk to Extension connection
  (Fixed, Cordless and IP)
- Extension to Extension connection

as well as in a vice versa connection.

In respect to a duration of 1 hour, this results in a maximum traffic of 48 Erlang at a Grade of Service (GOS) of 1,5%.

#### Trunk capacity

The maximum number of trunks is defined by the following parameters:

- Memory available in the system
  this limits to a theoretical maximum of 120 trunks
- Free slots for boards available in the system
  dependent on the configuration. For detailed information see Capacity Overview.
- Physical capacity on BP128i.
  The maximum amount of RJ45 sockets per cabinet is 72. This is shared between extensions, trunks, basestations, etc.

#### Extension capacity

The maximum number of extensions is defined by the following parameters:

- Memory available in the system, this limits to a theoretical maximum of 300 extension
- Free slots for boards available in the system dependent on the configuration. For detailed information see Capacity Overview.
- Relation between number of extension and number of trunks. This is very much dependent on the customer configuration. E.g. in Hotel installations the number of extensions compared to the number trunks will be much higher, whereas in Call Centers it will be much lower.
- Physical capacity on BP128i.
  The maximum amount of RJ45 sockets per cabinet is 72. This is shared between extensions, trunks, basestations, etc.

#### Capacity Overview

Devices | BP50 | BP128i | BP250 | Modularity
Extension Capacity (theoretical) | 300 | 300 | 300 | -
Extension Capacity (typical) | 64 | 128 | 200 (300 for Hotel systems) | -
| Digital | 8 - 64 | 8 - 128 | 8 - 200 (300 for Hotel systems) | 8/16/32
| Analog | 4 - 32 | 4 - 128 | 4 - 300 (300 for Hotel systems) | 4/8/16
| Cordless | 1 - 64 | 1 - 64 | 1 - 210 | defined by FECU
| Operator | 1 - 3 | 1 - 3 | 1 - 3 | 1
| S-interface Terminals | 1 - 64 (8 x 2B+D) | 1-128 (16 x 2B+D) | 1-192 (24 x 2B+D) | 4/8 x 2B+D
| H.323 clients | 200 | 200 | 200 | -
| CT monitored extensions | 80 (Office) 40 (Call Center) | 80 (Office) 40 (Call Center) | 80 (Office) 40 (Call Center) |
| Mobile | 100 | 100 | 100 | 5/20/40 +5
Trunk Capacity (theoretical) | 120 | 120 | 120 | -
Trunk Capacity (typical) | 30 | 60 | 60 |
| Analog trunk | 4 - 16 | 4-32 | 4 - 60 | 4/8
| Digital trunk PRA | 30 (1 x 30B+D) | 60 (2 x 30B+D) | 60 (2 x 30B+D) | 30 (1 x 30B+D)
| Digital trunk with CAS | 30 (1 x 30B+D) | 60 (2 x 30B+D) | 60 (2 x 30B+D) | 30 (1 x 30B+D)
| Digital trunk BA | 16 (8 x 2B+D) | 32 (16 x 2B+D) | 48 (24 x 2B+D) | 4/8 (4/8 x 2B+D)
| S-interface Terminals | 16 (8 x 2B+D) | 32 (16 x 2B+D) | 48 (24 x 2B+D) | 4/8 (4/8 x 2B+D)
| H.323 trunks | 30 | 60 | 60 | 4
| VoIP lines | 4-64 | 4-64 | 4-64 | 4/8/16
| Analog tie line | 4 - 8 | 4-16 | 4 - 56 | 4/8
Base Station | 12 | 12 | 60 | 1
Free slots for PBA´s (except CPU‑D5, CPU‑D4) | 4 | 4 + 5 | 8 + 9 + 9 | -
RJ45 sockets available | N/A | 72+72 | N/A | -

### Telephones

#### Digital telephones

Maximum line length |  | 800m with 0,5mm diameter |
typical cable impedance |  | 180W / 75 nF per km |

#### ISDN S-Interface

The S-interface complies with ETSI and AUSTEL supporting:

- Telefax Group 4
- PC with ISDN board
- PC with ISDN board and telephone
- Terminal adapter
- Videophone
- ISDN telephone

Supported bearer services are speech, unrestricted 64 kbits, unrestricted digital information (with tones/announcements 7kHz), 3.1kHz audio and video.

Ranges on the S-interface

Short passive bus |  | 250m |
Extended passive bus |  | 500m |

#### Analog telephones

Maximum loop resistance |  | 2500 W incl. telephone |
Current feed |  | 2 x 400 W, -48 VDC 2 x 800 W, -48 VDC |
Impulse speed |  | 10 Hz ±10% |
Make/break ratio |  | 33/67 - 40/60 ms |
DTMF-signalling |  | CCITT Q.23 |
Timed loop break (flash) |  | 80 - 120 ms |
Leakage resistance |  | 40 kW |

### Door interface unit

The wiring length between exchange and DIU should not exceed 500 m and between door phone and DIU not more than 50 m (applies for 0,5 mm diameter).

#### Speaker

impedance |  | 40...100 W |
nom. output |  | 20 mW at 50 W for - 10 dBm on a,b wires |
max. output |  | 200 mW / 50 W |

#### Microphone

impedance |  | 300 W |
DC feeding |  | 6 V / 330 W |
sensitivity |  | 15 mVeff with - 20 dBm on a,b wires |

#### Relay for door opener

Switching capability: 1,5 A / 48 VAC and 60 VDC

#### Environmental conditions

See Electrical characteristics.

### Trunks

#### Analog trunk

Maximum loop resistance |  | 2000 W at -48VDC |
Make/break ratio |  | 33/67 or 40/60 ms |
DTMF-signalling |  | CCITT Q.23/Q.24 |

#### Digital trunks

##### ISDN Basic Access

CE regulation |  | R&TTE 1999/5/EC |
CE marking |  |  |
ISDN signalling according to |  | CCITT I.430, I.440, I.450, I.441, I.451, ETSI CTR3 and Australian specification |

##### ISDN Primary Rate:

CE regulation |  | R&TTE 1999/5/EC |
CE marking |  |  |
ISDN signalling according to |  | CCITT I.431, I.440, I.450, I.441, I.451, G.703, G.704, ETSI CTR4 and Australian specification. |
Channel-associated signalling (CAS) R2 according to |  | CCITT Q421-424 |

### Tie lines

#### 2-wire analog tie line with DC-loop signalling

Maximum loop resistance |  | 2500 W |
Make/break ratio |  | 33/67 or 40/60 ms |
DTMF-signalling |  | CCITT Q.23/Q.24 |

#### 2/4 wire analog tie line with E&M signalling

Maximum loop resistance |  | 1800 W |
Maximum current for 0 W line |  | 9.0 mA |
Resistance in short-circuited M-loop |  | <35 W |
Maximum current in M-loop |  | 100 mA |

### Voice over IP lines / IP Extensions/ IP Networking

Ethernet Interface |  | 10BaseT/100BaseTX autosense LAN environment according to IEEE-802.3 for half-duplex and full-duplex operation |
Voice codecs: |  | G.711, G723.1, G.729 Annex A (with Annex B) |
Quality of Service |  | Type of Service (priorisation of voice packets) in the IP header |
Protocols |  | IPv4, vendor specific Operation an maintenance protocols, BOOTP, coding of speech packets according to RTP, DHCP, TCP, UDP, FTP, H.323 V4 (with support of Annex M.1), H.225, H.245, proprietary trunk gateway protocol |

### Transmission data

#### Coding

CCITT G.711, 8 bit PCM A-law

#### System impedance

600 W or programmable network/market specific impedances for analog interfaces.

#### 2-wire interfaces

- Return loss figure 1/Q.552

- 300-500 Hz: ³14 dB
- 500-2000 Hz: ³18 dB
- 2000-3400 Hz: ³14 dB

- Frequency distortion w. frequency

- Complies with ITU-T recommendation fig. 5/Q.552

- Group delay distortion w. frequency

- Complies with ITU-T recommendation fig. 6/Q.552

- Impedance unbalanced about earth

- Better than ITU-T recommendation fig. 2/Q.552

- Variation of gain w. input level

- Complies with ITU-T recommendation fig. 4/Q.552

- Cross talk

- Far-end and near-end cross talk between two connections in accordance with ITU-T Q.552/ 3.1.4.1 and 3.1.4.2

- Weighted noise

- Q.552/3.2.2.1.1 Output connection: better than ‑67 dBm0p for output rel. levels Lo>=-5dBr
- Q.552/3.2.2.1.1 Input connection: better than ‑65.2 dBm0p for equipment with signalling on speech wires

- Total distortion, including quantizing distortion

- In accordance with ITU-T recommendation fig. 12/Q.552 and fig. 13/Q.552

#### 4-wire interfaces

- Loss distortion w. frequency

- Complies with ITU-T recommendation fig. 4/Q.553

- Group delay distortion w. frequency

- Complies with ITU-T recommendation fig. 5/Q.553

- Impedance unbalanced about earth

- Better than ITU-T recommendation fig. 2/Q.552

- Variation of gain w. input level

- Complies with ITU-T recommendation fig. 4/Q.552

- Cross talk

- Far-end and near-end cross talk between two connections in accordance with ITU-T Q.552/ 3.1.4.1 and 3.1.4.2

- Weighted noise

- Q.552/3.1.3.1 Output connection: better than ‑70 dBm0p for signalling on separate wires
- Q.552/3.2.2.1.1 Input connection: better than ‑67 dBm0p signalling on separate wires

- Total distortion, including quantizing distortion

- In accordance with ITU-T recommendation fig. 10/Q.553 and fig. 11/Q.553

### CTI

#### V.24 interface:

V.24 interface |  | proprietary communication protocol |

#### Baudrate:

BusinessPhone BusinessLink Windows |  | 19200 Baud |

### Networking

#### QSIG standards

Basic Call Control |  | ETS 300 172 / ISO 11572, ISO 11574 |
GFP (within the scope of the supported supplementary service listed below ) |  | ETS 300 239 / ISO 11582 |
CLIP, COLP, CLIR |  | ETS 300 173 / ISO 14136 |
CNIP, CONP, CNIR |  | ETS 300 238 / ISO 13864, ISO 13868 |
AOC |  | ECMA 211/212 |
IP Networking |  | H.323 Annex M.1 |

#### Protocol compliance

Layer 1: |  | ETS 300 011 / ETS 300 012 |
Layer 2: |  | ETS 300 170 |
Layer 3: |  | ETS 300 172. |

### DECT Radio Interface

CE regulation: |  | 73/23/EEC, 89/336/EEC and 91/263/EEC respective 1999/5/EC |
CE marking: |  |  |
Frequency band: |  | 1880 -1900 MHz |
RF carriers: |  | 1897.344 MHz n*1.728 MHz (0 x n x 9) |
Number of carriers: |  | 10 |
Carrier spacing: |  | 1.728 MHz |
DECT standard: |  | CTR6 and CTR10 |
Power spectrum: |  | equal to GFSK with BT = 0.5 |
Frequency deviation: |  | as per CTR6 |
Peak output power: |  | 22 ±2 dBm |
Output spurious: |  | as per CTR6 |
Harmonics: |  | as per CTR6 |
Receiver sensitivity: |  | typical -83 dBm with a B.E.R. = 10-3 at the radio interface |
Unwanted emissions: |  | as per CTR6 |
Transmission: |  | MC/TDMA/TDD (Multiple Carrier/Time Division Multiple Access/Time Division Duplexing) |
TDMA frame: |  | 10 ms |
TDMA slot: |  | 0.417 ms |
No. of slots per frame: |  | 16 (8 full duplex channels) |
Total number of channels: |  | 120 |
Bit rate: |  | 1152 kbit/s |
Speech coding: |  | 32 kbit/s ADPCM (Adaptive Differential Pulse Code Modulation) |
#### Base Station
CE regulation: |  | 73/23/EEC, 89/336/EEC and 91/263/EEC |
CE marking: |  |  |
Operating voltage: |  | 12 to 56 VDC |
Power consumption: |  | 3.0 W typical (7.5 W peak) |
Output power: |  | 19 to 24 dBm |

### Compliance Information

ASB 150 02 is in conformity with Directives, Standards and other Normative Documents as listed.

- 73/23/EEC, Low Voltage Directive (LVD).
- 89/336/EEC, Electromagnetic Compatibility Directive (EMC)
- 1999/5/EC, Radio Equipment and Telecommunications Terminal Equipment Directive (R&TTE).

For details see
http://www.ericsson.com/enterprise/library/sdoc.shtml

Revision: Z © Ericsson Enterprise 2004