BusinessPhone Communication Platform 6.0
Commands > Commands 5000...5999

## 5213
Voice Mail CTI Access Code

This command allows to program a voice mail CTI access code, which is used by an external CTI application for control of the voice mail system.

The voice mail CTI access code is up to 4 digit and allows access and manipulation of all voice mails stored in the voice mail system.

##### Valid data

4 digits |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004