BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0x44
Unexpected NAK From E2

Default definition: |  | ERROR + TRIG |
Used by block: |  | ALL |
Category: |  | DESIGNER |

This code is used to inform OM about a NAK from the E2 handler.

- D1:
- D2: Error code from E2 (W = a warning is also done by the E2 handler)

- 01h: Write fail-error at verification reading (W).
- 02h: The input queue to the E2-handler is full (W) or a needed additional OS-buffer is not available.
- 04h: The record number is above the limit (W).
- 05h: No E2-record with the specified record number found.
- 06h: An identical identity code has been found (E2BASSZ).
- 07h: A specified E2 base area was not found.
- 08h: No free E2 memory (E2BASSZ or E2RECSZ).
- 09h: An identical directory number has been found (E2BASSZ).
- 0Ah: The base areas have different types (E2BASSWAP).
- 0Bh: Init aborted, E2 not available (W).
- 0Ch: Illegal parameter(s) found (E2RD or E2WR) (W).
- 0Dh: No space for more E2 base records.

- D3: Undefined
- D4: Undefined

Revision: I © Ericsson Enterprise 2004