BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0144
Hot line delay time

This command is used to give the time for delayed Hot line. This time is also used as time for activating of alarm if the Hot line number is the number to the alarm block (*53#).

Programming of hot line extension see command 0116 Hot line destination.

##### Valid data

0 |  | (default) |
1-250 |  | seconds |

Note

0 seconds corresponds to a not delayed Hot line, it corresponds to a normal Hot line.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004