BusinessPhone Communication Platform 6.0
Dialogs

## System Communication Statistics

This dialog is used to display statistical information about the communication channel, used by the selected board.

Each peripheral board can either use the High Speed Communication Channel (HSSC) or the Serial Communication Channel (SerCom). Additionally the message format (Format1 or Format2) as well as the maximum message length, used by the peripheral board, are included in the header of this dialog.

| Value
Card | Shows all available cards in the system.
Switched to | Used communication channel. (HSSC or SerCom)
Message Format | Used message format.
Message Length | Maximum message length.
HSSC Error | High Speed Communication Channel Errors
HSSC Frame Rx1 | High Speed Communication Channel Frame Receive 1.
HSSC Frame Tx1 | High Speed Communication Channel Frame Transmission 1.
HSSC Frame Rx2 | High Speed Communication Channel Frame Receive 2.
HSSC Frame Tx2 | High Speed Communication Channel Frame Transmission 2.
CMD 1 |
CMD 2 |
SerCom Error | Serial Communication Channel Errors
SerCom Message Rx | Serial Communication Channel Message Receive.
SerCom Message Tx | Serial Communication Channel Message Transmission

#### Actions

Submit |  | To submit your changes to the system. |
Reset |  | To reset the statistics of the selected board. |

Revision: B © Ericsson Enterprise 2004