BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0193
Automatic Redial allowed?

This command defines if an extenstion is allowed to use the feature "Automatic Redial" of external number.

Note

Operators always will be allowed to use the function automatic redial. Analog and cordless instruments, which do not support function keys, will be able to use the feature “Automatic Redial”via an interface to a CTI (Computer Telephony) application.

##### Valid data

Yes |  | (default) |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004